
For standalone installation,

    - Login as root. (You must be root in order to apply the update.) 

    - Place the Smart Component (CPxxxxxx.zip) in a temporary directory 

    - From the same directory, unzip the Smart Component:
               unzip CPxxxxxx.zip

    - Ensure that the file CPxxxxxx.vmexe is executable.
      Execute the commmand:

	chmod +x CPxxxxxx.vmexe

    - To perform the standalone installation, execute the command: 

             ./CPxxxxxx.vmexe 

    - Follow the directions given by the Smart Component 

    - If instructed, reboot your system for the firmware update to take effect 

