
FILE NAME:	CP028018.txt 

TITLE:	HPE QLogic NX2 Online Firmware Upgrade Utility for VMware Esxi

VERSION:    1.12.43

REVISION:	0

LANGUAGE:	English

CATEGORY:	Software Solutions

DIVISIONS:	Enterprise and Mainstream Servers

EFFECTIVE DATE: 9/21/2016

SUPERSEDES:	1.12.42



Products Affected
==================
HP Ethernet 10Gb 2-port 530FLR-SFP+ Adapter
HP NPAR 10Gb 2-port 530FLR-SFP+ Adapter
HP Flex-10 10Gb 2-port 530FLB Adapter
HP NPAR 10Gb 2-port 530FLB Adapter
HP Flex-10 10Gb 2-port 530M Adapter
HP NPAR 10Gb 2-port 530M Adapter
HP Ethernet 10Gb 2-port 530SFP+ Adapter
HP NPAR 10Gb 2-port 530SFP+ Adapter
HP Ethernet 10Gb 2-port 530T Adapter
HP NPAR 10Gb 2-port 530T Adapter
HP FlexFabric 10Gb 2-port 534FLB Adapter
HP NPAR 10Gb 2-port 534FLB Adapter
HP FlexFabric 10Gb 2-port 534FLR-SFP+ Adapter
HP NPAR 10Gb 2-port 534FLR-SFP+ Adapter
HP FlexFabric 10Gb 2-port 534M Adapter
HP NPAR 10Gb 2-port 534M Adapter
HP StoreFabric CN1100R Dual Port Converged Network Adapter
HP NPAR CN1100R Dual Port Converged Network Adapter
HP FlexFabric 10Gb 2-port 533FLR-T Adapter
HP NPAR 10Gb 2-port 533FLR-T Adapter
HP FlexFabric 20Gb 2-port 630FLB Adapter
HP NPAR 20Gb 2-port 630FLB Adapter
HP FlexFabric 20Gb 2-port 630M Adapter
HP NPAR 20Gb 2-port 630M Adapter
HP FlexFabric 10Gb 2-port 536FLB Adapter
HP NPAR 10Gb 2-port 536FLB Adapter
HPE StoreFabric CN1100R-T Converged Network Adapter
HPE NPAR 10Gb DP CN1100R-T
HPE FlexFabric 10Gb 4-port 536FLR-T Adapter
HPE NPAR 10Gb QP 536FLR-T
HPE 3820C 10/20Gb Converged Network Adapter
HP NPAR 3820C 10/20Gb Converged Network Adapter
HPE Synergy 10Gb 2-port 2820C Converged Network Adapter
HPE NPAR 10Gb 2-port 2820C Converged Network Adapter

Operating Systems
==================
Esxi 5.1
Esxi 5.5
Esxi 6.0
Esxi 6.5

Pre-requisites
===============
None

Description
============
This package contains the utilities and binaries for upgrading firmware (boot code, PXE, UEFI, iSCSI, NCSI, FCoE and CCM code) on HP Ethernet networking adapters (QLogic NX2 controller based) connected to supporting Proliant servers running supported VMware platform.

This component contains combo image version 7.14.79. The combo image includes: MFW: v7.13.75; PXE: v7.14.5; UEFI: v7.14.65; iSCSI(wherever applicable): v7.14.0 FCoE(wherever applicable): v7.14.3; L2: v7.12.25; CCM: v7.14.3.
The users will only see the combo image versions in the interactive mode firmware update or while using HPSUM/SPP to update the firmware on the supported adapters.

Enhancements/Fixes
===================
 - Enhancements Description:
     - Add support for 'HPE FlexFabric 10Gb 4-port 536FLR-T Adapter', 'HPE NPAR 10Gb QP 536FLR-T', 'HPE Synergy 3820C 10/20Gb Converged Network Adapter' & 'HP NPAR 3820C 10/20Gb Converged Network Adapter'.
   
 - Fixes Description:
  - Fixes an issue where the iSCSI and FCoE configuration menus show up even after enabling NPAR. 
  - Fixes an issue where the network devices may not show up in the Legacy BIOS Boot Order menu. 


Table of Contents
=================
Introduction
Packaging
Performing the Firmware Upgrade
Firmware Upgrade Log

Introduction
============
This file describes the procedure to use for upgrading firmware on HPE Ethernet networking adapters mentioned in the 'PRODUCTS AFFECTED' section of this document.

User guides and additional HPE network adapter information can be found at:
http://h18004.www1.hp.com/products/servers/networking/index-nic.html

 
Packaging
=========
The firmware upgrade utility is released in scexe format. The file is a single self-extracting executable that unpacks the component, runs it, and cleans up.

Performing the Firmware Upgrade
===============================
Off-line: 
-------	
SPP Off-line mode boots a special Linux OS environment, thus the Linux Smart Components are used, not the VMware Smart Components  

Remote On-line: If the component is supported by HP SUM but is not yet part of an SPP:
---------------
Download the appropriate SPP	
Add the component to the SPP	
Mount the SPP on a remote server running Windows or Linux that has a network connection to the ESXi host to be updated
Run HP SUM	
Add the ESXi host to be updated as a remote target/node 
Enter IP or DNS address of the ESXi host to be updated 
Enter the ESXi host credentials (root or administrator username and password) 
For HP SUM 6.0 and newer, select both the Additional Package with the added component and the SPP Baseline on the node Inventory page.
Follow HP Smart Update Manager Steps to complete the firmware update
Refer to the SPP documentation for detailed instructions at:www.hp.com/go/spp 

To use HP Insight Control for vCenter: 
-------------------------------------
Log in to the vSphere Client 	
Select a server or cluster in the inventory tree 
Click the HP Insight Management tab	
Follow Insight Control for vCenter steps to update firmware using a Smart Component 

To update firmware from VMware ESXi operating system on target server: 
---------------------------------------------------------------------
 - Enable Tech Support Mode on the ESXi host					
 - Login as root. (You must be root in order to apply the update) 					
 - Place the Smart Component zip file in a temporary directory					
 - Unzip the file CPXXXXXX.zip	
 - Ensure that CPXXXXXX.vmexe is executable by using the command:
 - chmod  +x  CPXXXXXX.vmexe				
 - From the same directory, execute the Smart Component. For example: ./CPXXXXXX.vmexe 					
 - Follow the directions given by the Smart Component 					
 - Logout					
 - Disable Tech Support Mode on the ESXi host	

Firmware Upgrade Log
====================
Results of the firmware upgrade are written to /var/cpq/CPxxxxxx.log.

Important Information
======================
1) The Device ID in NPAR (NIC Partitioning) mode is different over the DID used for Flex10, or (forced) Single Function mode. Accordingly adapters with DID 0x168E
and 0x16A2 changes to 0x16AE and 0x16A4 respectively after enabling NPAR.

Copyright 2016 Hewlett Packard Enterprise Developement LP.
Product names mentioned herein may be trademarks and/or registered trademarks of their respective companies.